<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.0">
<drawing>
<library>
<packages>
<package name="A-NIXIECLASSIC">
</package>
</packages>
<symbols>
<symbol name="A-NIXIE">
<description>Arduino Nixie clock board from www.nixieclock.biz
Classic Rev6</description>
<pin name="K0" direction="out"/>
<pin name="K9" direction="out"/>
<pin name="K8" direction="out"/>
<pin name="K7" direction="out"/>
<pin name="K6" direction="out"/>
<pin name="K5" direction="out"/>
<pin name="K4" direction="out"/>
<pin name="K3" direction="out"/>
<pin name="K2" direction="out"/>
<pin name="K1" direction="out"/>
<pin name="A10H" direction="out"/>
<pin name="A1H" direction="out"/>
<pin name="A10M" direction="out"/>
<pin name="A1M" direction="out"/>
<pin name="A10S" direction="out"/>
<pin name="A1S" direction="out"/>
<pin name="DATA0" direction="out"/>
<pin name="TICK_LED1" direction="out"/>
<pin name="TICK_LED2" direction="out"/>
<pin name="DP" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="RAW_VIN" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="170V" direction="pas"/>
<pin name="DLS" direction="in"/>
<pin name="BTN1" direction="in"/>
<pin name="PIR" direction="in"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="A-NIXIE">
<description>"Arduino" Nixie board from www.nixieclock.biz - Classic.

For creating a "hat/shield" display board which fits on top.

Elevated header sockets which work: 
Samtec ESQ-1xx-44-L-S, where xx is the number of pins.</description>
<gates>
<gate name="G$1" symbol="A-NIXIE"/>
</gates>
<devices>
<device name="" package="A-NIXIECLASSIC">
<connects>
<connect gate="G$1" pin="170V" pad="SV1-4"/>
<connect gate="G$1" pin="A10H" pad="SV3-6"/>
<connect gate="G$1" pin="A10M" pad="SV3-4"/>
<connect gate="G$1" pin="A10S" pad="SV3-2"/>
<connect gate="G$1" pin="A1H" pad="SV3-5"/>
<connect gate="G$1" pin="A1M" pad="SV3-3"/>
<connect gate="G$1" pin="A1S" pad="SV3-1"/>
<connect gate="G$1" pin="BTN1" pad="SV2-3"/>
<connect gate="G$1" pin="DATA0" pad="SV6-1"/>
<connect gate="G$1" pin="DLS" pad="SV2-2"/>
<connect gate="G$1" pin="DP" pad="SV6-4"/>
<connect gate="G$1" pin="GND" pad="SV1-3 SV2-1" route="any"/>
<connect gate="G$1" pin="K0" pad="SV5-1"/>
<connect gate="G$1" pin="K1" pad="SV5-2"/>
<connect gate="G$1" pin="K2" pad="SV5-3"/>
<connect gate="G$1" pin="K3" pad="SV5-4"/>
<connect gate="G$1" pin="K4" pad="SV5-5"/>
<connect gate="G$1" pin="K5" pad="SV5-6"/>
<connect gate="G$1" pin="K6" pad="SV5-7"/>
<connect gate="G$1" pin="K7" pad="SV5-8"/>
<connect gate="G$1" pin="K8" pad="SV5-9"/>
<connect gate="G$1" pin="K9" pad="SV5-10"/>
<connect gate="G$1" pin="PIR" pad="SV2-4"/>
<connect gate="G$1" pin="RAW_VIN" pad="SV1-2"/>
<connect gate="G$1" pin="TICK_LED1" pad="SV6-2"/>
<connect gate="G$1" pin="TICK_LED2" pad="SV6-3"/>
<connect gate="G$1" pin="VCC" pad="SV1-1 SV2-5" route="any"/>
</connects>
<technologies>
<technology name="">
<attribute name="REV" value="6"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
